# Release Notes for MFXSTM32L152 Component Drivers

Copyright © 2015 STMicroelectronics

# License

Licensed by ST under BSD 3-Clause license (the "License"). You may not use this package except in compliance with the License. You may obtain a copy of the License at:

https://opensource.org/licenses/BSD-3-Clause

# Purpose

This directory contains the MFXSTM32L152 component drivers.

# Update History

V2.0.3 / 03-April-2019

## Main Changes

- Update release notes format

V2.0.2 / 25-October-2018

## Main Changes

- Reformat the BSD 3-Clause license declaration in the files header (replace license terms by a web reference to OSI website where those terms lie)

V2.0.1 / 02-June-2017

## Main Changes

- Update comments to be used for PDSC generation

V2.0.0 / 24-June-2015

## Main Changes

- Add Shunt management of MFXSTM32L152 component
  - new mfxstm32l152_IDD_ConfigShuntNbLimit() and mfxstm32l152_IDD_GetShuntUsed() APIs
- Add mfxstm32l152_WriteReg() API

NOTE This release must be used with BSP Common driver V4.0.0 or later

V1.2.0 / 28-April-2015

## Main Changes

- mfxstm32l152_IO_Config(): remove unnecessary delay
- mfxstm32l152_TS_DetectTouch(): improve TouchScreen speed
- mfxstm32l152_IDD_Config(): add configuration of number of measure to be performed, with delay between 2 measures

NOTE
This release must be used with BSP Common driver V3.0.0 or later

V1.1.0 / 10-February-2015

## Main Changes

- Low Power management of MFXSTM32L152 component:
  - New mfxstm32l152_DeInit() and mfxstm32l152_WakeUp() API
  - mfxstm32l152_LowPower() API completed to be MFXSTM32L152 in Standby mode

NOTE
This release must be used with BSP Common driver V2.2.0 or later

V1.0.0 / 05-February-2014

## Main Changes

- First official release of MFXSTM32L152 IO Expander component driver.

NOTE
This release must be used with BSP Common driver V2.1.0 or later